{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":127,"n_cols":6,"rows_kept":127,"merged":[[0,1,0,5],[1,0,1,5],[2,0,2,5],[100,0,100,5]],"flags":["formulas_cached_only"]}
[null,"化材学院基础实验低值易耗品"]
["安师大化材学院2018-2019学年第二学期玻璃仪器、小型设备招标清单"]
["玻璃仪器"]
["序号","名称","规格","单位","数量","备注"]
[1,"26号细铁丝","30-36cm/根","包",2,"100根/包"]
[2,"3mm直径玻碳盘电极","上海辰华CHI104","根",3]
[3,"CR4级冷轧钢板","CR4级冷轧钢板（150*70*1mm，圆角R=3mm）","块",300]
[4,"USB延长线","1米","根",4]
[5,"石棉网","15cm包边","片",100]
[6,"饱和甘汞电极","上海辰华CHI150","根",5]
[7,"表面皿","9cm","个",20]
[8,"不锈钢药匙","1*3","套",100]
[9,"不锈钢长勺","30cm","把",80]
[10,"布氏漏斗","80mm","个",50]
[11,"布氏漏斗（带橡皮塞）","10mL","个",30]
[12,"层析柱","内径3cm","个",10,"磨口"]
[13,"冲击样条（聚丙烯）","80*10*2.5mm","个",1000]
[14,"冲击样条（聚乙烯）","80*10*2.5mm","个",1000]
[15,"磁子","A100","个",400]
[16,"磁子","A200","个",800]
[17,"磁子","A300","个",300]
[18,"打孔器","1*7","套",6]
[19,"导气弯管","19#","个",20,"磨口"]
[20,"滴管","L=15cm","根",1000]
[21,"滴瓶","60mL","个",100]
[22,"碘量瓶","250mL","个",60]
[23,"电极线","辰华CHI660系列工作站连接线--4接头","根",7]
[24,"分水器",null,"个",40,"磨口"]
[25,"粉末涂料漆膜试验板","150*70*厚度","片",400,"带孔"]
[26,"封口熔点毛细管","0.9-1.1*100mm","盒",10]
[27,"鼓泡吸收瓶",1904,"套",12,"玻璃"]
[28,"广口瓶","125mL","个",80]
[29,"广口瓶","60mL","个",100]
[30,"核磁管刷",null,"个",50]
[31,"核磁样品管",null,"个",30]
[32,"恒压滴液漏斗","60mL","个",20,"磨口"]
[33,"缓冲球","（旋转蒸发仪用24#转19#）","个",3,"磨口"]
[34,"碱式滴定管","50mL","支",50]
[35,"精密试纸","0.5-5.5","本",5]
[36,"空心塞（19#/90）","19#/90","个",80,"磨口"]
[37,"冷凝管夹",null,"个",60]
[38,"梨形烧瓶","19#/25mL","个",20,"磨口"]
[39,"量杯","500mL","个",5]
[40,"量筒","30cm×2.6cm","个",30,"特质，不需要刻度"]
[41,"量筒","10mL","个",200]
[42,"罗氏泡沫仪",2151,"套",2,"不带支架"]
[43,"点样毛细管","0.5*100mm","筒",15]
[44,"点样毛细管","0.3*100mm","筒",10]
[45,"毛细管","0.5*100mm","筒",10,"一端封口"]
[46,"容量瓶","250mL","个",100]
[47,"容量瓶","500mL","个",50]
[48,"容量瓶","1000mL","个",50]
[49,"容量瓶","10mL","个",100]
[50,"容量瓶","100mL","个",200]
[51,"三口烧瓶","100mL","个",30,"磨口"]
[52,"三口烧瓶","250mL","个",20]
[53,"砂纸","1200目","张",500]
[54,"烧杯","200mL","个",200]
[55,"烧杯","1000mL","个",72]
[56,"烧杯","150mL","个",200]
[57,"烧杯","250mL","个",200]
[58,"烧杯","50mL","个",600]
[59,"烧杯","100mL","个",800]
[60,"烧杯","500mL","个",72]
[61,"烧杯刷","小号","个",100,"50-100mL烧杯用"]
[62,"烧瓶夹",null,"个",200]
[63,"烧瓶刷",null,"个",300]
[64,"生料带",null,"卷",10]
[65,"试管","15*150mm","支",1400]
[66,"试管架（聚四氟乙烯）",null,"个",20]
[67,"试管刷","小号","个",300]
[68,"试管刷","大号","个",400]
[69,"小口试剂瓶","3000mL","个",6]
[70,"小口试剂瓶","30L","个",2]
[71,"小口试剂瓶","250mL","个",50]
[72,"小口试剂瓶","125 mL","个",100]
[73,"小口试剂瓶","25 mL","个",100]
[74,"数据线","串口线，DB9孔(母)-DB9孔(母) ","根",2]
[75,"塑料盒","内侧15cm*20cm*6cm","个",5]
[76,"塑料漏斗","下口径2.5cm，上口径18.5cm","个",3]
[77,"尾接管","19#","只",10]
[78,"吸量管","25mL","个",50]
[79,"吸量管","50mL","个",20]
[80,"洗耳球","大号","个",50]
[81,"洗瓶","500mL","个",200]
[82,"橡胶锤",null,"把",15]
[83,"新仪MAS-IIPlus型微波反应器四口反应瓶","500mL","个",10,"上海新仪配套件"]
[84,"新仪MAS-IIPlus型微波反应器四口反应瓶","100mL","个",10,"上海新仪配套件"]
[85,"液相进样针","平头，20微升","个",4]
[86,"液相进样针","100微升","个",4]
[87,"圆底烧瓶（19#/100ml）","19#/100mL","个",80,"磨口"]
[88,"圆底烧瓶（19#/250ml）","19#/250mL","个",30,"磨口"]
[89,"圆底烧瓶（19#/25ml）","19#/25mL","个",50,"磨口"]
[90,"圆底烧瓶（19#/50ml）","19#/50mL","个",90,"磨口"]
[91,"长滴管","L=30cm","支",20]
[92,"蒸馏头","19#","个",10]
[93,"锥形瓶","100mL","个",100]
[94,"紫外II型光谱照相版","9*24cm","盒",3]
[95,"玻璃反应釜  ","2500ml","个","6个","看样定制"]
[]
["小型设备"]
["序号","名称","参数、型号","单位","数量","备注"]
[1,"盘式粉碎机","ф175*磨盘直径:φ175mm; *给料粒度:≤4mm; *出料粒度:≤0.15mm; *生产率:25kg/h","台",1]
[2,"滚轴式罐磨机","PM-8-T适应物料<15mm; *出料粒度<0.0001mm, *附钢罐、陶瓷罐及钢和陶瓷研磨球与锻等研磨介质","台",3]
[3,"颗粒表面形态形貌分析仪","1.量程范围： 1um-3000um*2.系统放大倍数：4000倍。3.最小分辨率：0.1um4.重复性误差：<3%5.数字摄像头(CCD)：500万像素，分辨率2592×1944，像素尺寸2.2µm×2.2µm。*6.自动分割成功率：> 93%*7.软件能够自动标定颗粒的尺寸，自动分割粘连颗粒，自动分析，具有多幅图片合并及连续自动处理和分析的功能。可在图片中嵌入标尺，可以显示所有颗粒的粒形，测出长径比，球形度及粒度报告。8.配品牌电脑和打印机","套",2]
[4,"砼收缩膨胀仪","HSP-540*测量范围 534～545mm; *标准杆长度 540±0.2mm; *千分表量程 0～10mm; *外形尺寸（长×宽×高） 670×240×180mm","台",4]
[5,"砼压力泌水仪","SY-2","台",2]
[6,"胶砂试模","三联水泥胶砂，钢制40*40*160","套",10]
[7,"砼抗裂试模","铸铁425*305*100","套",5]
[8,"水泥砂浆干缩试模","标配铜质测头25*25*280mm，另配6×5个铜测头","套",5]
[9,"水泥砂浆干缩试模","标配铜质测头40*40*160mm，另配6×5个铜测头","套",5]
[10,"胶砂限制膨胀率仪","BC156-300/BC-Ⅱ测量范围156mm-305mm数显12.7mm千分表","套",5]
[11,"螺旋测微仪","数显，精度0.001mm  量程0-25mm","套",5]
[12,"实验室小推车","不锈钢双层，550*370*850mm，无噪音","个",2]
[13,"实验室静电粉末喷涂机（打样静电喷枪）","1，数字显示电压，直观；2，智能型操作界面：为方便使用者可通过触摸式按键选择相应的模式（a.凹角模式，适合喷涂复杂形状及凹角部位时;b.重喷模式，用于因排斥静电不易涂装或者再次涂装时;c.平板模式） \n机器参数：\n输入电压: 110V-220V；频率: 50-60Hz；输入功率:50W；最大输入气压: 8公斤；最小输入气压:4公斤；压缩空气最大水汽含量:1.3g／立方米；最大压缩空气消耗量：10立方米／h；出粉量：500g／min（5bar时）；离子极性：负极；粉杯容粉量：400克。\n","套",2,"杭州卡罗弗喷涂设备有限公司实验型静电粉末喷枪COLO-800DT-06C"]
[14,"浮标式氧气吸入器","YH.YX11D ","个",2,"上海医疗器械股份有限公司"]
[15,"工具套装","含（锂电钻、羊角锤、万用表、活动扳手、卷尺、剥线钳、水管钳、老虎钳、尖嘴钳、内六角扳手、锯子、精密批*4、棘轮手柄、一字起子、十字起子等）淘宝价格为368元","套",1,"闽豹"]
[17,"电动橡胶塞打孔器","02006/1-13mm","台",1]
[18,"加湿器","美菱MH-260","台",1]
[19,"磁力加热套","250mL","台",10]
[20,"电热套","不带调压,100ML","个",30,"河南巩义仪器设备有限公司"]
[21,"调压器","TDGC2-1,调压范围0-250V","台",20,"浙江天正电器股份有限公司"]
[22,"恒温水油浴锅","R201D，功率1.2KW","个",5,"杭州大卫科教仪器有限公司"]
[23,"博世（BOSCH） 锂电手电钻GSB120家用电动螺丝刀电动手动工具","gsb120-li双电+108件套","套",1]
[24,"手持式抛光机",null,"台",1]
[25,"水泵全自动清洗机",null,"台",1]
[26,"夹式台灯放大镜","带灯2.25倍维修放大镜","台",3]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}